Config: -

|  |  |
| --- | --- |
| **Overview** | Attempt to access Vicon data on personal Linux machine |
| **Goal** | Transferring Vicon data from the windows machine to the Linux machine through Ethernet |
| **Next Steps** | * Attempt to do the same thing with a hotspot or wifi instead of Ethernet * SSH connection to Modal AI drone to find out essential information |
| **Notes** | * MX1 IP: 192.168.10.1 * MX2 IP: 192.168.10.2 * Personal Linux Machine IP: 192.168.10.3 * On C++ code set the host as the MX2 IP |